­October 2016

Re: Potential LEED credits for projects (based on LEED-NC, version 2.1)

To whom it may concern:

Babcock-Davis certifies and provides the following information for use in achieving LEED-NC credit for the specification of Babcock-Davis Entrance Mats and Grilles.

Product: **alumaGRIL™ Rigid Grille**

Model(s): **BGA10**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LEED Category | Credit | Details | Points | Product/Material Detail |
| Material and Resource(MR) | 4 | Recycled Content: Post-consumer +1/2Pre-consumer content | 1 to 2possible points | Minimum:* 52% pre-consumer
* 15% post- consumer recycled content
 |
| 5 | Regional material: Use building materials or products that have been extracted, harvested or recovered, as well as manufactured, within 500 miles of the project site | 1 to 2possible points | Extraction Point is:* Brampton, ON

Final Packaging Facility Location:* Pickering, ON
 |
| Indoor Environmental Quality (EQ) | 4.1 | Low-Emitting Materials – Adhesives and Sealants | 1 possible point | Not applicable |
| 4.2 | Low-Emitting Materials – Paints and Coatings | 1 possible point | Not applicable |
| 4.3 | Low-Emitting Materials – Flooring Systems | 1 possible point | Not applicable. Product does not require adhesives or sealants in the field. |
| 5 | Indoor Chemical and Pollutant Source Control: Employ permanent entryway systems at least 10 feet long in the primary direction of travel to capture dirt and particulates entering the building at regularly used exterior entrances. Acceptable entryway systems include permanently installed grates, grilles and slotted systems that allow for cleaning underheath. Roll-out mats are acceptable only when maintained on a weekly basis by a contracted service organization. | 1 possible point | Meets the requirement if size of product is at least ten (10) feet in the traffic direction and the product is properly maintained. |

If you require any further information, please do not hesitate to contact us.