­April 2018

Re: Potential LEED credits for projects (based on USGBC LEED, version 4)

Babcock Davis certifies and provides the following information for use in achieving LEED-NC credit for the specification of Babcock Davis Floor Doors.

Product: **Drainable, aluminum, Pedestrian Load Floor Door, Single and Double Leaf**

Model(s): **BFDDPA**

|  |  |  |
| --- | --- | --- |
| LEED Category | Details | Product/Material Detail |
| **Material and Resource**(MR): Building Product Disclosure- Sourcing of Raw Materials. | Recycled Content: Post-consumer + ½ Pre-consumer content | Contains 40% pre-consumer and 30.5% post-consumer recycled content. |
| Point of Extraction | Extraction point is not within 500 miles of manufacturing.Final Packaging Facility Location:* Brooklyn Park, MN
 |
| **EQc2** Low Emitting Materials |  | MSDS Provided  |

|  |  |  |  |
| --- | --- | --- | --- |
| **BFDDPA\_X\_SFL + BFDDPA\_X\_DFL** | **Pre-Consumer** | **Post-Consumer** | **Weight / SF (lbs.)** |
| **Total Weight** |  |  | **1** |
| Aluminum Door + Door Components | **81.2%** | **0.0%** | **0.42** |
| Aluminum Frame + Frame Components | **10.00%** | **65.00%** | **0.40** |
| SST Hinges + Hardware | **11.25%** | **25.00%** | **0.18** |
|  Odor Gasket | **0.00%** | **0.00%** | **.00** |
| **% Recycled Content Aluminum Door** | **34.1%** | **0%** |  |
| **% Recycled Content Aluminum Frame** | **4%** | **26%** |  |
| **% Recycled Content Stainless Steel** | **2.03%** | **4.5%** |  |
| **Total % Recycled Content - Based on Weight** | **40.03%** | **30.5%** |  |
| **Total Recycled Content (Post Consumer + 1/2 Pre-Consumer)** |   | **50.5%** |