RE: Sustainability Statement

Babcock-Davis certifies and provides the following information for use in achieving LEED v4 credit for the specification of Babcock-Davis Entrance Mats.

**Product** MatDesign™ Aluminum Hinge Roll-up Mats

**Models:** BMD38P, BMD38R, BMD38V, BMD38G, BMD38X, BMD38E, BMD38U, BMD38B

**Manufacturing Info**

* Final Assembly Location: Brooklyn Park MN
* Extraction point is not within 500 miles of manufacturing
* Recycled Content
	+ BMD38Pand BMD38R contain
		- 37% pre-consumer, 19% post-consumer recycled content.
	+ BMD38V
		- 29% pre-consumer, 14.5% post-consumer recycled content.
	+ BMD38E
		- 50.7% pre-consumer, 21.7% post-consumer recycled content
	+ BMD38U
		- 35% pre-consumer, 17.7% post-consumer recycled content.
	+ BMD38G
		- 37% pre-consumer, 18% post-consumer recycled content.
	+ BMD38B
		- 31% pre-consumer, 16% post-consumer recycled content.
* Health Product Declaration – Not available.

**LEED Credit Options:**

* EQ Credit: Enhanced Indoor Air Quality Strategies
	+ Option 1. Enhanced IAQ Strategies (1 point)
		- Entryway Systems: Install permanent entryway systems at least 10 feet (3 meters) long in the primary direction of travel to capture dirt and particulates entering the building at regularly used exterior entrances. Acceptable entryway systems include permanently installed grates, grilles, slotted systems that allow for cleaning underneath, rollout mats, and any other materials manufactured as entryway systems with equivalent or better performance. Maintain all on a weekly basis.

If you require any further information, please do not hesitate to contact us at (888) 412-3726.

##