**MAXgrid® Flexible MAT**

**Models: BMG12**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **LEED Category** | **Credit** | **Details** | **Points** | **Product/Material Detail** |
| Material and Resources (MR) | 4 | Recycled Content: Post-consumer + ½ Pre-consumer content | 1 to 2 possible points | Post-consumer 0%  Pre-consumer 0% |
| 5 | Regional Material: Use building materials or products that have been extracted, harvested or recovered, as well as manufactured,  within 500 miles of the project site | 1 to 2 possible points | Not applicable |
| Indoor Environmental Quality (IEQ) | 4.1 | Low-Emitting Materials—Adhesives and Sealants | 1 possible point | Not applicable. |
| 4.2 | IE Q Credit 4.2: Low-Emitting Materials—Paints and Coatings | 1 possible point | Not applicable. |
| 4.3 | Low-Emitting Materials—Flooring Systems | 1 possible point | Not applicable. Product does not require adhesives or sealants in the field. |
| 5 | Indoor Chemical and Pollutant Source Control: Employ permanent entryway systems at least 10 feet long in the primary direction of travel to capture dirt and particulates entering the building at regularly used exterior entrances. Acceptable entryway systems include permanently installed grates, grill s and slotted systems that allow for cleaning underneath. Roll-out mats are acceptable only when maintained on a weekly basis by a contracted service organization. | 1 possible point | Meets the requirement if size of product is at least ten (10) feet in the traffic direction and the product is properly maintained. |