January 1, 2019

RE: Roof Hatch Safety Grab Bar Product Change Notice

Babcock-Davis announces the release of our updated Roof Hatch Safety Grab Bars to Safety Yellow Powder Coat.

Additions to the design:

* + New Aluminum rail and gate construction
	+ Light weight design allows for easier and faster installation
	+ Fits all brands of roof hatches that have a counterflash
	+ Safety yellow powder coat finish standard
	+ Still provides a non-penetrating attachment to the hatch via the counterflash
	+ 5 year warranty

Specifications:

* + Rails / Posts – Aluminum pipe, 1-1/4 inch (31 mm) ID (1.66 inch OD) Schedule 40, 6061 T6 alloy
	+ Fittings – Aluminum alloy 5052-H32
	+ Mounting brackets – 3/16 inch steel, zinc plated
	+ Hardware – Hex head bolts 3/8 inch – 16 by 34 inch zinc plated steel

|  |  |  |
| --- | --- | --- |
| **MODEL** | **MATERIAL** | **FINISH** |
| BSGBAY | Aluminum | Powder Coat, Safety Yellow |

The new aluminum safety rail and gate will begin shipping January 1, 2019. Please contact us at 1.888.412.3726 should you have any questions or concerns. We appreciate the opportunity to service you.

­