January 1, 2019



RE: Roof Hatch Safety Railing Product Change Notice

Babcock-Davis announces that powder coat safety yellow is now standard on all Roof Hatch Safety Railings.

**Features**

* + Aluminum rail and gate construction
	+ Light weight design allows for easier and faster installation
	+ Meets OSHA 29 CFR 1926.502
	+ Available in standard and custom sizes, fits all brands of roof hatches that have a counterflash
	+ Non-penetrating attachment to the hatch via the counterflash
	+ Five (5) year warranty

**Specifications**

* + Rails / Posts: Aluminum pipe, 1-1/4 inch (31 mm), schedule 40, 6061 T6 alloy
	+ Fittings: Aluminum alloy 5052-H32
	+ Gate: Aluminum pipe, 1-1/4 inch (31 mm), schedule 40, 6061 T6 alloy
	+ Mounting brackets: 3/16 inch steel, zinc plated

|  |  |  |
| --- | --- | --- |
| **Standard Sizes****(W x L)** | **Standard Hatch** **with Gate** | **Thermally Broken Roof Hatch with Gate** |
| 36” x 30” | BSRCAY36X30FG | BSRBAY36X30FG |
| 36” x 36” | BSRCAY36X36FG | BSRBAY36X36FG |
| 48” x 48” | BSRCAY48X48FG | BSRBAY48X48FG |
| 30” x 54” | BSRCAY30X54SG | BSRBAY30X54SG |
| 30” x 72” | BSRCAY30X72SG | BSRBAY30X72SG |
| 30” x 96” | BSRCAY30X96SG | BSRBAY30X96SG |

The new powder coat safety yellow aluminum safety rails will begin shipping January 15, 2019. Please contact us at 1.888.412.3726 should you have any questions or concerns. We appreciate the opportunity to service you.

­