**QuietFlex® LDPE Hinge Roll-Up Mats**

**Models: M-650, M-650U, M-650RS, M-750, M- 750ET, M-750RT, M-850, M-950, M-1050**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **LEED Category** | **Credit** | **Details** | **Possible Points** | **Product/Material Detail** |
| Material and Resources (MR) | 4 | Recycled Content: Post-consumer + ½ Pre-consumer content | 1 to 2 possible points | * M-650, M-650U and M-650RS contain 29% pre-consumer and 14% post-consumer recycled content.
* M-750 contains 22% pre-consumer and 11% post-consumer recycled content.
* Model M-750ET contains 37.2% pre-consumer, 43.3% post consumer recycled content
* M-750RT contains 32% pre-consumer and 16% post-consumer recycled content.
* M-850 contains 28% pre-consumer and 14% post-consumer recycled content.
* M-950 and M-1050 contain 35% pre-consumer and 17% post-consumer recycled content.
 |
| 5 | Regional Material: Use building materials or products that have been extracted, harvested or recovered, as well as manufactured, within 500 miles of the project site | 1 to 2 possible points | Not applicable. Extraction Point is not within 500 miles of manufacturing. Final Packaging: Brooklyn Park, MN 55428 |
| 6 | Rapidly Renewable Materials: Use rapidly renewable building materials and products for 2.5% of the total value of all building materials and products used in the project, based on cost. Rapidly renewable building materials and products are made from agricultural products that are typically harvested within a 10-year or shorter cycle. | 1 possible point | Not applicable.  |
| Indoor Environmental Quality (IEQ) | 4.3 | Low-Emitting Materials—Flooring SystemsAll carpet installed in the building interior must meet the testing and product requirements of the Carpet and Rug Institute Green Label Plus1 program.All carpet adhesive must meet the requirements of IEQ Credit 4.1: Adhesives and Sealants, which includes a volatile organic compound (VOC) limit of 50 g/L. | 1 possible point | Not applicable. Product does not require adhesives or sealants in the field. |
| 5 | Indoor Chemical and Pollutant Source Control: Employ permanent entryway systems at least 10 feet long in the primary direction of travel to capture dirt and particulates entering the building at regularly used exterior entrances. Acceptable entryway systems include permanently installed grates, grill s and slotted systems that allow for cleaning underneath. Roll-out mats are acceptable only when maintained on a weekly basis by a contracted service organization. | 1 possible points | Meets the requirement if product is installed at least ten (10) feet in the direction of traffic and properly maintained. |