January 1, 2019



RE: Floor Door Safety Railing Product Change Notice

Babcock-Davis announces that powder coat safety yellow is now standard on all Floor Door Safety Railings.

**Features**

* + Aluminum rail and gate construction
	+ Light weight design allows for easier and faster installation
	+ Meets OSHA 29 CFR 1926.502
	+ Available in standard and custom sizes
	+ Five (5) year warranty

**Specifications**

* + Rails / Posts: Aluminum pipe, 1-1/4 inch (31 mm), schedule 40, 6061 T6 alloy
	+ Finish: Safety Yellow Powder Coat
	+ Fittings: Aluminum alloy 5052-H32
	+ Gate: Aluminum pipe, 1-1/4 inch (31 mm), schedule 40, 6061 T6 alloy
	+ Mounting brackets: 3/16 inch steel, zinc plated

The new powder coat safety yellow aluminum safety rails will begin shipping January 1, 2019. Please contact us at 1.888.412.3726 should you have any questions or concerns. We appreciate the opportunity to service you.

­