February 2018

Re: Potential LEED credits for projects (based on USGBC LEED, version 4)

Babcock Davis certifies and provides the following information for use in achieving LEED-NC credit for the specification of Babcock Davis Entrance Floor Mats + Grilles.

Product: **alumaGRIL™**

Model(s): **BGL10B, BGL10P, BGL10R, BGL10S, BGL10W**

|  |  |  |
| --- | --- | --- |
| LEED Category | Details | Product/Material Detail |
| **Material and Resource**  (MR): Building Product Disclosure- Sourcing of Raw Materials. | Recycled Content:  Post-consumer + ½ Pre-consumer content | Contains 64.6% pre-consumer and 6.7% post-consumer recycled content. |
| Point of Extraction | Extraction point is not within 500 miles of manufacturing.  Final Packaging Facility Location:   * Brooklyn Park, MN |
| **EQc2** Low Emitting Materials |  | Not applicable. No finishes, sealants or adhesives in product ingredients. |
| **EQc4** Indoor Air Quality Assessment |  | Meets the requirement if length of product is (10) feet in the direction of traffic |

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Pre-Consumer** | **Post-Consumer** | **Weight** |
| **Total Weight** |  |  | **1** |
| **Aluminum Rails** | **68%** | **7.0%** | **.95** |
| Zinc Plated Steel Support Bars | **0%** | **0%** | **.05** |
| **% Recycled Content (*Based on Weight*)** | **64.6%** | **6.7%** | **1** |
|  |  |  |  |
| **Total % Recycled Content - Based on Weight** | **64.6%** | **6.7%** | **1** |
|  |  |  |  |
|  |  |  |  |
| **Total Recycled Content (Post Consumer + 1/2 Pre-Consumer)** | | | **39.0%** |