­June 2017

Re: Potential LEED credits for projects (based on LEED-NC, version 4)

To whom it may concern:

Babcock-Davis certifies and provides the following information for use in achieving LEED-NC credit for the specification of Babcock-Davis Safety Rails.

Model(s): **SRCA, SRBA, SGBA**

|  |  |  |
| --- | --- | --- |
| LEED Category | Details | Product/Material Detail |
| Material and Resource  (MR): Building Product Disclosure- Sourcing of Raw Materials. | Recycled Content: Post-consumer +1/2  Pre-consumer content | Aluminum: 65%  Contains 9.5% pre-consumer and 61% post-consumer recycled content. |
| Point of Extraction | Extraction point is not within 500 miles of manufacturing.  Final Packaging Facility Location:   * Brooklyn Park, MN |

If you require any further information, please do not hesitate to contact us.