­June 2017

Re: Potential LEED credits for projects (based on LEED-NC, version 4)

To whom it may concern:

Babcock-Davis certifies and provides the following information for use in achieving LEED-NC credit for the specification of Babcock-Davis Roof Hatches.

Products: **ThermalMAX™**

Model(s): **BRHTA**

|  |  |  |
| --- | --- | --- |
| LEED Category | Details | Product/Material Detail |
| Material and Resource(MR): Building Product Disclosure- Sourcing of Raw Materials. | Recycled Content: Post-consumer +1/2Pre-consumer content | Aluminum: 65%Contains 9.5% pre-consumer and 61% post-consumer recycled content. |
| Point of Extraction | Extraction point is not within 500 miles of manufacturing.Final Packaging Facility Location:* Brooklyn Park, MN
 |

If you require any further information, please do not hesitate to contact us.